

|  |  |  |
| --- | --- | --- |
| Pairs of poles | SW5  | SW6 |
| 2 | ON | OFF |
| 4 | OFF  | ON  |
| 5 | ON  | ON  |
| Default setting | OFF | OFF |

Open loop: SW7=ON

Closed loop: SW7=OFF

Closed loop mode(useless when SW7=ON):

SW8=ON closed loop for current

SW8=OFF closed loop for speed and current